JULY 28, 2026
SECTION 06 42 00 – TIMBERLAB RESOLVE GLT™ / non-structural GLued-laminated wood panel

1. GENERAL
0. RELATED DOCUMENTS
0. Drawings and general provisions of the Contract, including General and Supplementary Conditions and Division 01 Specification Sections, apply to this Section.
SUMMARY
Section Includes:
TIMBERLAB RESOLVE GLT™
Field finishing
Related Requirements:
{Specifier’s Note: Keep relevant sections below depending upon how the TIMBERLAB RESOLVE GLT™ is being used on the project.}
Section 01 81 13 “Sustainable Design Requirements”.
Section 05 12 00 “Structural Steel Framing” for coordination with structural steel frame (when used as a beam/column wrap).
Section 06 10 00 "Rough Carpentry" for substrates, nailers, and blocking.
[bookmark: _Hlk58313952]Section 06 40 00 “Architectural Woodwork” for coordination with other architectural panels.
[Section 09 91 00 “Painting” for field finishing of glued-laminated panels.]
[Section 09 93 00 “Staining and Transparent Finishing” for field finishing of glued-laminated panels.]
DEFINITIONS
TIMBERLAB RESOLVE GLT™: A non-structural glued-laminated (Glulam) wood panel; intended for finish/aesthetic use only.
AOR: Architect of Record hired by the project owner or the Design-Build General Contractor.
REFERENCES
AWI 200 – Care & Storage
ANSI/AWI 0642 – 2024 – Wood Paneling
[ASTM D7612- Standard Practice for Categorizing Wood and Wood-Based Products According to Their Fiber Sources, 2021.]
SUBMITTALS
Product Data: For each type of product.
Include product data on lumber and adhesives.
Panel dimensions, tolerances, and profile details.
For field-applied sealing product, include product data and application instructions.
Samples: Provide a minimum of three samples, with minimum dimensions of 12-inch by 12-inch, for each species combination demonstrating the range of variation to be expected in appearance of non-structural glued-laminated panels.
[bookmark: _Hlk56774267]Samples will be supplied unfinished from manufacturer.
[bookmark: _Hlk58353374]{Specifier’s Note: Retain Sustainable Design Submittals language below only for Projects pursuing LEED® green building program certification (under version 4.1) or revise text for other sustainable design certification programs.}
Sustainable Design Submittals: Refer to Section 01 81 13 “Sustainable Design Requirements”.
LEED®[footnoteRef:1] green building program MR Credit 3 - Sourcing of Raw Materials: [1:  LEED – an acronym for Leadership in Energy and Environmental Design™ - is a registered trademark of the U.S. Green Building Council®.   |   usgbc.org/LEED] 

Certified Wood: Documentation indicating percentage new wood, percentage Forest Stewardship Council® (FSC)[footnoteRef:2] and Chain-of-Custody (CoC) certificates for manufacturer and vendor. Include vendor invoice indicating FSC® and CoC. [2:  FSC® Chain of Custody: SCS-COC-007899   |   Trademark: FSC-C162183  |   fsc.org/en
] 

[bookmark: _Hlk57714664]Pilot Alternative Compliance Path - Legal Wood: Documentation of wood products from Certified Sources as defined by ASTM D7612 meeting following requirements:
100 percent of all wood is verified to be from Legal (non-controversial) Sources as defined by ASTM D7612. 
70 percent of all wood used on the Project is from Responsible Sources as defined by ASTM D7612. 
{Specifier’s Note: Retain Sustainable Design Submittals language below only for Projects pursuing LEED certification (under version 5.0) or revise text for other sustainable design certification programs.}
0. Sustainable Design Submittals: Refer to Section 01 81 13 “Sustainable Design Requirements”.
LEED MR Credit 4 – Building Product Selection and Procurement   
Submit product documentation necessary to score eligible products in accordance with USGBC’s approved LEED v5 MRc4 multi-attribute scoring methodology. TIMBERLAB RESOLVE GLT™ can earn LEED Multi-attribute points in the following areas:
{Specifier’s Note: When specifying reclaimed glulam, use the following potential points.}
· Recycled Content (1/2 x pre-consumer %) – 0.5 points for Circular Economy
· Wood Products: Legal Sourcing and Disclosure – 1 point for Ecosystem Health
{Specifier’s Note: When specifying virgin input fiber, use the following potential points.}
· Wood Products: Legal Sourcing and Disclosure – 1 point for Ecosystem Health
· Wood Products: “FSC Mix” label – 4 points (2 points for Ecosystem Health + 2 points for Social Health & Equity)
· Wood Products: “SFI® Certified Chain of Custody – Promoting Sustainable Forestry”[footnoteRef:3] label – 3 points (2 points for Ecosystem Health + 1 point for Social Health & Equity) [3:  SFI® Chain of Custody: SCS-SFI-COC-007899   |   Trademark: SFI-01976   |   forests.org       
   		*SFI marks are registered marks owned by the Sustainable Forestry Initiative Inc.] 

· Wood Products: “PEFC Certified”[footnoteRef:4] label – 3 points (2 points for Ecosystem Health + 1 point for Social Health & Equity) [4:  PEFC Chain of Custody: SCS-PEFC-COC-007899   |   Trademark: PEFC/29-31-395   |   www.pefc.org] 

QUALITY ASSURANCE
[bookmark: _Hlk74765528]TIMBERLAB RESOLVE GLT™ shall be factory-manufactured under controlled conditions.
Adhesives shall be specifically formulated for interior architectural woodwork, capable of producing a durable, uniform, and stable bond consistent with the fabrication and performance criteria required by AWI Standards for architectural woodwork and interior finishes.
DELIVERY, STORAGE, AND HANDLING
General: Comply with provisions in AWI 200 – Care & Storage.
TIMBERLAB RESOLVE GLT™ must be palletized for delivery and protected to prevent water intrusion.
Store flat, elevated from grade, under cover. Handle to prevent damage.
PROJECT CONDITIONS
Do not install TIMBERLAB RESOLVE GLT™ until building is enclosed, and ambient conditions are stabilized to service levels.
Acclimate panels for 48 hours minimum prior to use/installation.
Warranty
Manufacturer’s standard one-year warranty against defects in materials and fabrication, excluding natural wood color and grain variations and damage due to improper storage, handling, installation, or maintenance.
PRODUCTS
PERFORMANCE REQUIREMENTS
[bookmark: _Hlk57716387]{Specifier’s Note: Include applicable sustainability requirements for project.}
Sustainability Requirements: Comply with Section 01 81 13 “Sustainable Design Requirements”.
Manufacturer
Basis-of-Design Product: TIMBERLAB RESOLVE GLT™ by Timberlab.
Manufacturer: Timberlab Laminators, LLC. 850 NW 13th Ave, 5th Floor, Portland, OR 97209, Office Phone: (503) 749-7500
Substitutions: Not Permitted 
materials
Wood Species
{Specifier’s Note: Include Visual Face species options below as applicable.
Visual Face Species Options:
[Douglas Fir (DF)]
[Southern Pine (SYP)]
[Spruce Pine Fir (SPF)]
[Alaskan Cedar (AYC)]
Non-visual face and panel core composed of visual face species or Douglas Fir.
{Specifier’s Note: If project has FSC® or SFI requirements, use the appropriate line for Certiﬁed Wood below. Verify availability of FSC® and SFI certiﬁcation per species at time of pricing.} 
1. Certiﬁed Wood: Input glued laminated timber shall be certiﬁed as “FSC Mix Credit” according to FSC STD-01-001, “FSC Principles and Criteria for Forest Stewardship,” and to FSC STD-40-004, “FSC Standard for Chain of Custody Certiﬁcation.” 
Certiﬁed Wood: Input glued laminated timber shall be certiﬁed as “SFI Credit” or “SFI 100% as calculated under the credit method” according to “SFI 2022 Forest Management Standard” and to “SFI 2022 Chain of Custody Standard.” 
{Specifier’s Note: Reclaimed material from Timberlab’s glulam manufacturing facilities available in Douglas Fir and Southern Pine species. If specifying reclaimed wood, select the species below. Verify availability of reclaimed material per species at time of pricing.
[Reclaimed Wood: Use reclaimed Douglas Fir glued laminated timber from Timberlab’s glulam manufacturing facilities as input material when available.]
[Reclaimed Wood: Use reclaimed Southern Pine glued laminated timber from Timberlab’s glulam manufacturing facilities as input material when available.] 
Adhesives
Moisture‑resistant wood adhesives suitable for laminated wood panels.
TIMBERLAB RESOLVE GLT™ construction
Dimensions
Finished thickness: 0.75”
Thickness tolerance: ± 0.008 inches
Nominal panel size: 24” x 96”
Squareness tolerance: ±1/32 inch over panel width
Length/width tolerance: ±1/32 inch either direction
Configuration
Three ply panel
Each ply is a prepared wood lamination using lamellas cut from glued-laminated timber.
Cross laminated construction.
The first and third plies are oriented along the length of the panel.
The second (middle) ply is oriented along the width of the panel.
Panels shall have one visual face.
Edge Profile
Tongue on one long edge and one short edge.
Groove on the opposing long edge and short edge.
Tongue and groove orientation consistently aligned with the designated visual face and species.
finish
Finish Options:
Factory sanded (to 150 grit), unfinished.
Field applied finish (by others).
Apply finish per finish manufacturer’s instructions.
EXECUTION
EXAMINATION
Verify that furring and/or substrates in areas to receive TIMBERLAB RESOLVE GLT™ are plumb, flat, and within tolerances to achieve flush panel alignment. Report unsatisfactory conditions in writing.
Proceed with installation only after unsatisfactory conditions have been corrected.
PREPARATION
Refer to AWI 200 – Care & Storage for storage and protection prior to installation.
Coordinate furring or backing/blocking in conditions where panels are used to wrap structural steel beams or other structural members.
INSTALLATION
Installation by others.
Install per approved submittals, and in accordance with the construction documents and AWI Standards for installation tolerances and substrate penetration.
Maintain tongue-and-groove orientation consistent with designated visual face and layout specified by the AOR.
Installers to use fasteners suitable for installation of TIMBERLAB RESOLVE GLT™ to substrate, based on substrate construction.
Use stainless or coated fasteners compatible with finish.
Joints:
Shim, level, and align panels to produce flush, uniform joints consistent with AWI guidelines.
Maintain uniform joint widths and alignments and tight tongue-and-groove engagement.
Do not force joints; address substrate tolerances first.
Non-structural use; do not use panels to support imposed loads or as shear/diaphragm elements.
Joined surfaces should be sanded flush.
field finishing
When field finishing, sand and clean surfaces, and apply coatings per Division 09, matching approved samples.
PROTECTION
Protect installed TIMBERLAB RESOLVE GLT™ panels from damage and moisture during construction. Temporary edge guards are recommended.
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